Patch-ID# 114880-02
Keywords: sun ray update patch security
Synopsis: Sun Ray Server version 2.0 Patch Update
Date: Nov/25/2003


Install Requirements: Reboot after installation                      
                      
Solaris Release: 8 9

SunOS Release: 5.8 5.9

Unbundled Product: Sun Ray Server Software

Unbundled Release: 2.0

Xref: 

Topic: 

Relevant Architectures: sparc

BugId's fixed with this patch: 4369691 4433854 4781321 4792984 4810192 4810962 4813815 4817187 4825312 4825808 4828674 4833004 4834790 4836233 4838105 4838723 4839252 4839685 4840440 4841227 4841279 4841623 4841678 4842640 4842791 4844714 4855375 4858575 4863617 4874498 4877262 4878246 4881981 4890267 4894276 4898094 4907215

Changes incorporated in this version: 4878246 4838105 4834790 4898094 4858575 4855375 4781321 4907215 4863617 4877262 4890267 4792984 4881981 4894276 4369691

Patches accumulated and obsoleted by this patch: 

Patches which conflict with this patch: 

Patches required with this patch: 

Obsoleted by: 

Files included with this patch: 

/etc/opt/SUNWut/gulogin.start
/etc/opt/SUNWut/loginGUI.start
/etc/opt/SUNWut/sessionTypes.props
/opt/SUNWut/cgi-bin/desktop
/opt/SUNWut/lib/app-defaults/guloginGUI.res
/opt/SUNWut/lib/firmware/CoronaP1
/opt/SUNWut/lib/firmware/CoronaP2
/opt/SUNWut/lib/firmware/CoronaP3
/opt/SUNWut/lib/firmware/CoronaP4
/opt/SUNWut/lib/firmware/CoronaP5
/opt/SUNWut/lib/firmware/CoronaP6
/opt/SUNWut/lib/guloginGUI
/opt/SUNWut/lib/libutgrpmgr.so
/opt/SUNWut/lib/libutinfo.so.1
/opt/SUNWut/lib/libutscr.so.2
/opt/SUNWut/lib/libutsmon.so.1
/opt/SUNWut/lib/modules/Authxlation.jar
/opt/SUNWut/lib/modules/StartSession.jar
/opt/SUNWut/lib/modules/StartxlationSession.jar
/opt/SUNWut/lib/nscloginGUI
/opt/SUNWut/lib/pixmaps/GUdefault.xpm
/opt/SUNWut/lib/pixmaps/GUsunray.xpm
/opt/SUNWut/lib/scloginGUI
/opt/SUNWut/lib/sunray_get_user.so.1
/opt/SUNWut/lib/utauthd.jar
/opt/SUNWut/lib/utdtsession
/opt/SUNWut/lib/utgenpolicy
/opt/SUNWut/lib/utpamcfg
/opt/SUNWut/lib/utprefs-helper
/opt/SUNWut/lib/utresexec
/opt/SUNWut/lib/utseriald
/opt/SUNWut/lib/utxexec
/opt/SUNWut/lib/utxinit
/opt/SUNWut/sbin/utdesktop
/opt/SUNWut/sbin/utfwadm
/opt/SUNWut/sbin/utuser
/usr/lib/secure/libc_ut.so
/usr/lib/secure/sparcv9/libc_ut.so
/usr/openwin/server/modules/ddxSUNWsunray.so.1

Problem Description:

4369691 Frimware info displayed in GUI/CLI for DTU is confusing to user.
 
4781321 SunRay Module causes SunMC agent VM to grow
 
4792984 pam.conf update ignores existing pam entries for dtlogin/dtsession
 
4834790 Firmware returns wrong data for return code 0x63XX during an APDU transaction.
 
4838105 utuser -p $CORONA_TOKEN sometimes fails when raw token is JavaBadge
 
4855375 Load balancing takes too long to even out unbalanced load.
 
4858575 /usr/lib/libc_ut.so library's stat routine seg. faults at NULL file argument
 
4863617 ut_isServerAlive SEGFAULTS if server times out
 
4877262 GNC vulnerability in non-default session types
 
4878246 off-by-one memory write in library key/value code
 
4881981 Admin library calls use multithread unsafe system calls.
 
4890267 New Quatech SSU-100 devices (PID 0xC020) not working with SunRays
 
4894276 Sun Ray firmware responds to arbitrary multicast ping
 
4898094 Freed memory is being referenced later in the code.
 
4907215 utinfo::issuePropertiesCallback() should block for connected
 
(from 114880-01)
 
4433854 Sometimes smartcard removal is not detected and session stays active
 
4810192 X server rendering cleanup
 
4810962 A forceInsert on redirect should carry forward the redirectProps values
 
4813815 username property does not get carried along for redirects to non-trusted hosts
 
4817187 Minor mathematical manipulation mitigates multihead mouse mispositioning
 
4825312 CAM/kiosk session does not restart after logout on fast hardware
 
4825808 Javabadge smartcards are sometimes recogonized as OpenPlatform cards.
 
4828674 sunray_get_user.so does not work correctly if stacked multiple times
 
4833004 Determine the home server for a DTU
 
4836233 Lazy Authentication, authd should push authentication to as late as possible
 
4838723 Remove the acceptRedirectToken property from auth.props
 
4839252 SRSS2.0; outline of StarOffice window remains
 
4839685 X server drops to low bandwidth limit when packets are lost
 
4840440 postpatch script needs to handle LAN case for utfwadm
 
4841227 Bad processing after lost packet causes bad command interpretation
 
4841279 utfwadm -N all with no LAN subnets gives bogus errors
 
4841623 Need a new PAM module to get username infomation
 
4841678 utfwadm -A -a -N all does not work
 
4842640 Need utility interfaces for lazy auth (sunray_get_user)
 
4842791 Redirection from server doing encryption to one that's not fails
 
4844714 Add DHCP XDM option to specify Sun Ray server list
 
4874498 Sun/Fujitsu mouse rev(05c/06c) may fail to work in SunRay due to bad packets

Patch Installation Instructions:
-------------------------------- 
For Solaris 2.8 & 9 releases, refer to the man pages for instructions
on using 'patchadd' and 'patchrm' scripts provided with Solaris.
Any other special or non-generic installation instructions should be
described below as special instructions.  The following example
installs a patch to a standalone machine:
 
        example# patchadd /var/spool/patch/114880-02
 
The following example removes a patch from a standalone system:
 
        example# patchrm 114880-02
 
For additional examples please see the appropriate man pages.

Special Install Instructions:
----------------------------- 
 
Required Patches
----------------
 
Warnings & Errors
-----------------
** WARNING: This patch should only be applied to systems which
        have Sun Ray Server Software 2.0 fully installed.  Do not
        attempt to add this patch to the UFS image to be applied as
        part of the install process **
 
** WARNING: Unconfiguring the Sun Ray Server Software before
	removal of this patch may lead to error messages and/or
	removal failure 
 
** WARNING: Login behavior for Non-SmartCard Mobility sessions is
	slightly different, see the following section on LAN Security
	Enhancement.
 
LAN Security Enhancement
------------------------
LAN Security for Non-SmartCard Mobility (NSCM) has been improved, and this
results in a very slightly different user experience when logging in,
which users may wish to be prepared for.  The property
acceptRedirectTokens in /etc/opt/SUNWut/auth.props no longer exists.
Instead, normal login for NSCM now may redirect a user after the
username is entered and before the password-entry screen is presented.
This results in final authentication occurring on the server where the
user's session will be accessed or created.  This has two user-visible
effects, when contrasted to the previous default case where
acceptRedirectTokens=false:
 
	1. Users will never need to enter their username and password
	twice.
 
	2. After entering the username, the NSCM screen will disappear
	and some Sun Ray On Screen Display (OSD) icons will briefly
	appear while the Sun Ray is being redirected to the correct
	server, after which the NSCM screen for "Enter password" will
	appear.  Note that type-ahead will no longer function during
	this interval.  The user must now wait for the password-entry
	screen to be drawn before typing their password.
 
It is hoped that this should not present a significantly different
login experience to users, while providing increased security.
 
 
Sun Ray Firmware Upgrades
-------------------------
 
This patch includes firmware updates for Sun Ray appliances.  The
updated firmware will be loaded by your Sun Ray appliances through the
usual Sun Ray firmware download mechanism.  The firmware changes are
independent of the Sun Ray Server Software changes but are delivered
in this patch for your convenience.
 
If this patch is being applied to servers configured into a Sun Ray
failover group it must be applied to all servers in the group at your
earliest convenience.  While some members of the group remain unpatched
the restart time of your Sun Ray appliances may be noticeably longer
than usual.  The increased restart time can be avoided by taking the
action described in step 1 below.
 
The following additional steps are required when adding this patch on a
live system:
 
        (before applying patch to system)
 
        1. (optionally) Suppress firmware downloads from all servers in
        a Sun Ray failover group
 
        2. Stop Sun Ray services on the server being patched
 
        (after applying patch)
        3. Reboot the Sun Ray server
 
 
To remove this patch, carry out these steps in the following order:
 
        (before removing the patch)
 
        1. (optionally) Suppress firmware downloads from all servers in
           a Sun Ray failover group
 
        2. Stop Sun Ray services on the server being patched
 
        (after removing the patch)
        3. Reboot the Sun Ray server
 
 
Detailed Steps
--------------
 
1. Suppress firmware downloads
 
        If the server being patched is not a member of a Sun Ray
        failover group you should skip this step.
 
        If the server being patched is a member of a Sun Ray failover
        group then this step is optional but is strongly recommended.
 
        At Patch Installation
        ---------------------
 
            Before adding this patch to servers configured into a Sun
            Ray failover group we advise that you disable Sun Ray
            firmware delivery from all unpatched hosts in the failover
            group.  On each host in the group:
 
                For each of the dedicated network interconnects:
 
                    $ /opt/SUNWut/sbin/utfwadm -a -D -n <intf>
 
                For each of the shared subnetwork interconnects:
 
                    $ /opt/SUNWut/sbin/utfwadm -a -D -N <subnetwork>
 
            Do this only one time, before adding this patch to any
            server in the group.
 
            The purpose of this step is to prevent unpatched servers
            from offering old firmware to Sun Ray appliances that have
            already accepted the new firmware delivered with this
            patch.
 
            If this patch is being applied to a Sun Ray failover group
            then omitting this step may result in increased restart
            times for your Sun Ray appliances.  (A mixture of patched
            and unpatched servers advertising conflicting firmware
            versions may cause the appliance to download new firmware
            each time it restarts.  The appliance automatically
            restarts itself after downloading fresh firmware so its
            overall restart cycle is longer in that case.  The
            appliance may restart itself several times before
            establishing or reconnecting to a session.)  The Sun Ray
            restart time will return to normal once the patch has been
            added to all servers in the failover group.
 
        At Patch Removal
        ----------------
 
            Before removing this patch from servers configured into a
            Sun Ray failover group we advise that you disable firmware
            delivery from any hosts in the failover group that have
            this patch installed.  On each already-patched host in the
            group:
 
                For each of the dedicated network interconnects:
 
                    $ /opt/SUNWut/sbin/utfwadm -a -D -n <intf>
 
                For each of the shared subnetwork interconnects:
 
                    $ /opt/SUNWut/sbin/utfwadm -a -D -N <subnetwork>
 
            Do this only one time, before removing this patch from any
            of the already-patched servers in the group.
 
            The purpose of this step is to prevent already-patched
            servers from offering new firmware to Sun Ray appliances.
 
            If this patch is being removed from a Sun Ray failover group
            then omitting this step may result in increased restart
            times for your Sun Ray appliances.  (A mixture of patched
            and unpatched servers advertising conflicting firmware
            versions may cause the appliance to download new firmware
            each time it restarts.  The appliance automatically
            restarts itself after downloading fresh firmware so its
            overall restart cycle is longer in that case.  The
            appliance may restart itself several times before
            establishing or reconnecting to a session.)  The Sun Ray
            restart time will return to normal once the patch has been
            removed from all servers in the failover group.
 
 
2. Stopping Sun Ray services and login sessions
 
        Before applying this patch to a Sun Ray server or removing this
        patch from a Sun Ray server all users should be logged out of
        their Sun Ray sessions.
 
        Stop the Sun Ray services using the following command:
 
                $ /etc/init.d/utsvc stop
 
        This command will terminate any Sun Ray sessions that were not
        already logged out.
 
        Next, add or remove the patch using the instructions outlined
        above in the section "Patch Installation Instructions".
 
        Adding the patch automatically prepares the server to advertise
        new firmware to your Sun Ray appliances.  Removing the patch
        automatically prepares the server to revert to advertising
        pre-patch firmware to your Sun Ray appliances.
 
 
3. Rebooting the Sun Ray server
 
        The Sun Ray server must be rebooted after the addition or
        removal of the patch.

README -- Last modified date:  Tuesday, November 25, 2003

