Patch-ID# 120881-04

NOTE:
***********************************************************************
READ THE TERMS OF THE AGREEMENT ("AGREEMENT") IN THE LEGAL_LICENSE.TXT
FILE CAREFULLY BEFORE USING THIS SOFTWARE. BY USING THE SOFTWARE, YOU
AGREE TO THE TERMS OF THIS AGREEMENT. IF YOU DO NOT AGREE TO ALL OF THE
TERMS, PROMPTLY DESTROY THE UNUSED SOFTWARE.
***********************************************************************

Keywords: sun ray update patch linux security jds2 rhelas3.0 sles8.0
Synopsis: Sun Ray Core Services version 3.1 JDS2 RHELAS3.0 SLES8.0 Patch Update
Date: Jul/20/2006


Install Requirements: Additional instructions may be listed below                      
                      
Solaris Release: 
Note: JDS RedHat SUSE


SunOS Release: 
Note: JDS2 RHELAS3.0 SLES8.0


Unbundled Product: Sun Ray Core Services

Unbundled Release: 3.1

Xref: This patch available for SUNOS 5.8 5.9 5.10 as 120879-04 and for 5.10_x86 as 120880-04

Topic: 

Relevant Architectures: i386

BugId's fixed with this patch: 5060424 6238984 6254552 6311482 6316937 6319180 6325171 6327741 6328992 6330608 6331518 6338007 6338019 6344009 6344241 6346040 6348306 6351087 6354210 6354786 6376242 6380565 6383912 6385918 6393502 6397106 6398942 6399779 6412036 6413607 6418906 6421484 6424125 6426377 6427681 6430465 6438243

Changes incorporated in this version: 6418906 6424125 6427681 6413607 6412036 6338019 6421484 6426377 6438243 6430465

Patches accumulated and obsoleted by this patch: 

Patches which conflict with this patch: 

Patches required with this patch: 

Obsoleted by: 

Files included with this patch: 


Note:	SUNWuta-3.1-32.21.i386.rpm
	SUNWutfw-3.1-32.21.i386.rpm
	SUNWutgsm-3.1-32.21.i386.rpm
	SUNWutkau-3.1-32.21.i386.rpm
	SUNWutm-3.1-32.21.i386.rpm
	SUNWuto-3.1-32.21.i386.rpm
	SUNWutps-3.1-32.21.i386.rpm
	SUNWutr-3.1-32.21.i386.rpm
	SUNWutu-3.1-32.21.i386.rpm

Problem Description:

6418906 sunray_get_user:isValidUsername logs too much information to syslog - security
6424125 AMGH is inefficient when Sun Ray is already in local FOG
6427681 AMGH can cause "rolling redirects" within a FOG
6413607 utdevctl fails on new firmware
6412036 utsettings can fail when run against some Sun Ray 2 firmware builds
6338019 Sun Ray needs to distinguish between Sun Type 6 Japanese keyboard and other Japanese keyboards
6421484 Sun Ray smartcard driver masks odd INS bytes
6426377 utgenpolicy SPOF - attempts to update primary DS, which can block authd startup
6438243 Mondex MM2 cards are not recognized
6430465 Admin Password cannot be changed from Admin GUI.
 
(from 120881-03)
6376242 utauthd core dump seen on  Solaris 8 system (also duplicate utauthd processes on running systems)
6380565 3rd party license readme distribution update
 
(from 120881-02)
6383912 utxconfig constrains X desktop dimensions to unreasonably low values
6351087 Regression: Xsun spins in Sun Ray DDX
6327741 pam.conf is not updated correctly causing login problems
6393502 Sun Ray firmware needs to report smartcard ATR history length as well.
6385918 SRSS needs to support Belgian eID smartcard
6397106 GemPlus GPK16000 cards and newer JCOP21 cards need to be supported
6331518 Sun Ray Server Software (SRSS) should support GEM+/GEM Expresso (64V2N) smartcards
6398942 TCP connections can fail when initialization sequence is irregular
6348306 Add tool to administer licenses
6399779 sometimes uttsc core dumps while hotdesking
 
(from 120881-01)
6319180 utxconfig is insufficently paranoid
6238984 utseriald dumps core after resetting the DTU connected with serial adapter
6328992 utauthd eats 2 file descriptors when a fork fails
6325171 ndbm database corruption causes utdesktop and authd to core dump.
6316937 DTU hangs and power cycles when trying to send data using loopback cables with SR 170 embedded ports
6311482 Restart of Sun Ray services from Admin GUI using netscape7 is not working as expected
6346040 Update smartcard config files to work with new versions of cards
5060424 DTUs not getting configured MTU from LAN Sunray Server
6254552 ISO 7816-4 Case 1 APDU problem
6330608 2 authd running on the same box,  (parent and child) causing authd to hang and all DTU get 26 error
6354786 Restart not working from Admin GUI after patch installation.
6344009 Alt-tab doesn't work after they upgrade Sunray SW from 3.0 to 3.1
6344241 After upgrading from SRSS 3.0 to 3.1 the Num Lock and Shift keys don't work via IOGear KVM
6354210 Linux kernel audio driver returns EAGAIN on write() when it shouldn't
6338007 Xnewt exhibits pixmap security issue described by X.org, CAN-2005-2495

Patch Installation Instructions:
-------------------------------- 
NOTE: Before patch installation, make a copy of the auth.props file
      which will have to be copied back after patch installation.
 
      cp -p /etc/opt/SUNWut/auth.props <path_name>/auth.props-backup
 
To install this patch, run the following command for each RPM:
 
      rpm --nodeps -F --noscripts 'rpmname'
 
      Consult the rpm(1) man page for more details.
 
NOTE: After patch installation, restore the saved auth.props file.
 
      cp -p <path_name>/auth.props-backup /etc/opt/SUNWut/auth.props
 
      After patch installation and before rebooting the server,
      run the following commands to install the new audio driver
 
	# cd /usr/src/SUNWut/utadem
	# make clean
	# make
	# make install

Special Install Instructions:
----------------------------- 
NOTE: This patch is for the Sun Ray Core Services 3.1 component that is
part of Sun Ray Server Software 3.1.
 
NOTE: This SRSS patch does not support Live Upgrade.  Please do not
install this patch via live upgrade.
 
NOTE: Some third party terms were not included in the original version of 
Sun Ray Server Software 3.1 in the THIRDPARTYLICENSEREADME.html. This patch
includes a new THIRDPARTYLICENSEREADME.html that contains all the terms.
 
 
NOTE: The DTU firmware delivered in this patch has the following version
identification string
 
    3.1_120879-04_2006.06.22.15.58
 
Required Patches
----------------
 
Warnings & Errors
-----------------
** WARNING: This patch should only be applied to systems which have
	    Sun Ray Server Software 3.1 fully installed.  Do not attempt
	    to add this patch to the UFS image to be applied as part of
	    the install process **
 
** WARNING: This patch redelivers the 
	    /etc/opt/SUNWut/smartcard/probe_order.conf file.
	    If you have modified this file, the changes will be lost, and
	    you will need to make the same changes to the new copy.
 
 
 
 
Detailed Steps
--------------
 
1. Suppress firmware downloads
 
	If the server being patched is not a member of a Sun Ray
	failover group you should skip this step.
 
	If the server being patched is a member of a Sun Ray failover
	group then this step is optional but is strongly recommended.
 
	At Patch Installation
	---------------------
 
	    Before adding this patch to servers configured into a Sun
	    Ray failover group we advise that you disable Sun Ray
	    firmware delivery from all unpatched hosts in the failover
	    group.  On each host in the group:
 
		For dedicated network interconnects:
 
		    $ /opt/SUNWut/sbin/utfwadm -a -D -n all
 
		For shared subnetwork interconnects:
 
		    $ /opt/SUNWut/sbin/utfwadm -a -D -N all
 
	    Do this only one time, before adding this patch to any
	    server in the group.
 
	    The purpose of this step is to prevent unpatched servers
	    from offering old firmware to Sun Ray appliances.
 
 
2. Stopping Sun Ray services and login sessions
 
	Before the addition of this patch to a Sun Ray server
	all users should be logged out of their Sun Ray sessions.
 
	Stop the Sun Ray services using the following commands:
 
                $ /etc/init.d/utsvc stop
 
	These commands will terminate any Sun Ray sessions that were not
	already logged out.
 
	Next, use the instructions outlined above in the section
	"Patch Installation Instructions" for the addition
	of this patch.
 
	Adding the patch automatically prepares the server to advertise
	new firmware to your Sun Ray appliances.
 
 
3. Rebooting the Sun Ray server
 
	The Sun Ray server must be rebooted after the addition
	of the patch.
 
4. Enable firmware downloads
 
	After the addition of this patch on all Sun Ray
	servers in a failover group, enable firmware downloads
	using one of the following methods:
 
	1) If all Sun Ray server in the failover group provides firmware
	   downloads run this command on one of the servers:
 
		$ /opt/SUNWut/sbin/utfwsync
 
	   After which the Sun Ray DTU's will reboot themselves and load
	   the new firmware.
 
	2) If only some of the Sun Ray servers in the failover group provide
	   firmware downloads to the DTU's, run the following command
	   on the servers that do provide firmware:
 
	   For dedicated network interconnects:
 
		$ /opt/SUNWut/sbin/utfwadm -a -A -n all
 
	   For shared subnetwork interconnects:
 
		$ /opt/SUNWut/sbin/utfwadm -a -A -N all
 
	   Then restart services on all servers in the failover group by
	   executing the following command on a server in the group:
 
		$ /opt/SUNWut/sbin/utfwsync -d

README -- Last modified date:  Thursday, July 20, 2006

