######################################################
1. You need to have 2 USB cables:
######################################################

MTCDT:
======

a. The first USB cable will have to connect to the Conduit's debug port.

   See screen shot - usb-debug-cable-location

b. The second USB cable will have to connect to the USB device port on the back of the Conduit.

   See screen shot - USB-device-port-location

MTCDTIP:
========

a. See MTCDTIP-ReleaseB-DebugAndDevicePorts.

#####################################################
2. Install SAMBA util.

#####################################################

The SAM-BA utility for Windows is here:
--> http://www.microchip.com/DevelopmentTools/ProductDetails.aspx?PartNO=Atmel%20SAM-BA%20In-system%20Programmer


#####################################################
3. Download and unzip the firmware file

a. Make sure you have unzip the firmware file into your C:\ drive.


#####################################################
4. a. Plug in the Debug cable first and go to Uboot. To go into the Uboot,

      power cycle the unit and keep hitting the space bar on your PC until

      it goes into the Uboot. If you missed it, redo it again, and again...


   b. See screen shot from 1 to 6 (Be sure to read the comment in the screen shot too)


#####################################################

5. Plug in your second USB cable and flashing the firmware

#####################################################

a. See screen shot from 7 to 11 (Be sure to read the comment in the screen shot too)




