*****************************************************
* MTR-X Firmware 3.5.6 Release Notes                *
*****************************************************
Contents:
1) Models Covered By This Firmware.
2) Firmware Upgrade Procedure.
3) Engineering Release Notes for Customer.
4) Support Information.

****************************************************
*    Models Covered By This Firmware               *
****************************************************
- MTR-C2-x
- MTR-EV3-x
- MTR-G3-x
- MTR-H5-x
- MTR-H6-x
- MTR-LAT1-x
- MTR-LEU1-x
- MTR-LVW2-x

****************************************************
*    Firmware Upgrade Procedure                    *
****************************************************
Upgrading to 3.5.6.

Note: Backup your configuration before performing this upgrade. If the firmware upgrade fails,
or it does not show the login page again, wait an additional 5 minutes. Power off and on the MTR
and web to the MTR to check the version. If the version does not show the latest, then the
upgrade was not successful. Try to perform the firmware upgrade again by repeating all the steps.

NOTE:
To upgrade using the MTR Web UI to MTR 3.5.6 it is highly recommended that the device be running the MTR 3.4.5 firmware.
To upgrade from a previous firmware, upgrading to MTR 3.4.5 is necessary before upgrading to MTR 3.5.6.

1) Save the firmware binary file to a directory on your workstation.
2) Using the workstation browser, enter the IP address of the MTR (i.e. http://192.168.2.1).
3) Login as admin and enter the admin password.
4) Click "Administration" tab on left side menu bar.
5) Click "Save/Restore".
6) Click "Save Configuration to File" to save a backup file. A popup window will appear.
7) Select "Save File" and click "OK" button.
8) Now click "Firmware Upgrade" tab on left side menu.
9) Click the Browse button and select the latest version of BIN file, rcell-mtr-upgrade_3.5.6.bin
   or rcell-mtrv1-upgrade_3.5.6.bin.
10) Click the "Start Upgrade" button. Confirm the 5 minute "OK" button.
11) Wait for the unit to upgrade and reboot automatically.
12) Again, browse to the IP address and verify the Main or Home Page indicates the correct version, 3.5.5.

****************************************************
*    Engineering Release Notes for Customer        *
****************************************************
-----------------------------------------------------
MTR firmware 3.5.6 - November 2016
-----------------------------------------------------
Changes made since release 3.5.5:
- Fixed various Help issues.

Bug Fixes since release 3.5.5:
- Fixed IPv6 PPP-IP Passthrough on MTR-LVW2.
- Add Activation checks for MTR-EV3-x-N2 (Sprint) to delay PPP connections to avoid connection
  conflicts if MTR is not activated.

Known Issues in 3.5.6:
- On MTR-EV3, continuous ringing of Wake On Call prevents cellular wake up.

****************************************************
*      Support Information                         *
****************************************************
Multi-Tech provides free technical support for your product. To obtain this support,
we suggest you create a support case on our Support Portal at:
https://support.multitech.com

If internet is not available, try one of our numbers:
U.S. & Canada number: 763-717-5863
Answered Monday - Friday
8:00 am to 5:00 pm Central Time (Daylight savings observed when in effect)

International number: +763-717-5863
Answered Monday - Friday
8:00 am to 5:00 pm Central Time (Daylight savings observed when in effect)

EMEA    support@multitech.co.uk         +(44) 118 959 7774
U.S.    support@multitech.com           800-972-2439 or
(and Rest of World)                     +763-717-5863

Replacement Parts and Accessories
For replacement parts and accessories, contact Multi-Tech at:
(888) 288-5470, option 3 or +1 (763) 785-3500

US Mail Address:
  Multi-Tech Systems, Inc.
  2205 Woodale Drive
  Mounds View, MN 55112
  USA

::Form Version R2014-03-27::