HOW TO LOAD THE FIRMWARE FIX TO THE MULTIVOIP:


SERIAL METHOD:
-------------

1.Go to our web server and download the following file: 

  - 14.11.18-10-Jun-09.zip

  - http://www.multitech.com/en_US/SUPPORT/Families/MultiVOIPFX/firmware.aspx

2. Install the downloaded file into your PC. This is a MultiTech

   software for upgrade and configure the MultiTech device.

Note: Skip the above step if you already had it installed.


3. Go to our ftp server again and download the firmware fix:

   - 14.11.1B-15-Dec-11.zip

   - ftp://ftp.multitech.com/engineering/unofficial-releases/MultiVOIP/FX/14.11.1B


4. Unzip this zip file into a folder and make note of the folder where you have 

   it unzipped. We need it later.


5. Hook up a serial cable from the PC to the command port of the MultiVOIP 
 
   that you want upload the firmware fix to.


6. Click on start button -> Programs -> MultiVOIP xxx -> 

   Select Download firmware -> Open file dialog box comes up -> Click on 

   Browse button and browse to the folder in Step # 4. Select the file 

   named: mvpt1.bin and click Open button to download the firmware fix to

   the box.

7. When done, go into the System Info and verify that firmware version is:

   14.11.1B.


8. Test them out.

#####################################################################################
