MultiVOIP Firmware v6.11.41 November 30 2015

This firmware is for models MVP210, MVP410, and MVP810 and is based on the v6.11.22 firmware.

Changes and Bug Fixes since v6.11.22:
- Fixes for Web Interface compatibility issues with Java 8 and later versions.
- Added User Agent to SIP Registration packets.
- Added User Agent to SIP Options packets.
- Fixes a problem in E&M passthrough where the E and M lead changes weren't always updated correctly, 
  causing the remote side to occasionally be in the wrong state until the next change.


Note: When using Java 8, you may need to add the MultiVOIP to the Java Exception Site List. 
To do this go to Control Panel and select Java. When the Java Control Panel comes up, select the 
Security tab. Very that the Security level is set to High and click Apply if changed. Next click the
Edit Site List button, this should bring up the Exception Site List menu. Click the Add button, 
select the new location added in the list, add the MultiVOIP's address to the list with a http:// prefix
and press enter. An example of this would be "http://192.168.3.143". After pressing enter you will be
prompted with a security warning, click Continue to accept the location. Click OK to close the Exception 
Site List menu and again to close the Java Control Panel.

************************************************************************
NOTICE: This is a developmental test release created to address specific 
issues or requests that may or may not be merged into an official 
release at a later date. This developmental test release HAS NOT been 
thoroughly tested and functionality MAY CHANGE in a later release. By 
using this developmental test release you accept all liability and risk 
stemming from its use.
************************************************************************


Update Instructions
If installing using the MultiVOIP Software on a PC with a serial port follow the 
"MultiVOIP Software Upgrade" instructions, otherwise follow the "FTP Upgrade" instructions.


MultiVOIP Software Upgrade:
1. Install the MultiVOIP v6.11.22 Software, if not already installed. 
   This can be found at the link below.
   ftp://ftp.multitech.com/multivoip/6.11.22-11-Jun-09.zip

2. Connect the MultiVOIP to the PC serial port and power it on, if not powered
   on already. Note the USB to serial convertors may not work with MultiVOIP Software.
   When the boot light is off, go to the next step.

3. Run the MultiVOIP Software's "Configuration" before upgrading and take note of the current
   settings. Note the settings should be retained during the upgrade.

4. Unzip the "6_11_41-30_nov_2015.zip" file to a known location.

5. Run the MultiVOIP Software's "Download Firmware" and when prompted to select the "*.BIN"
   file, browse to the "6_11_41-30_nov_2015.bin" file you unzipped in the previous step and click open.

6. The Download Firmware process will take several minutes. When the MultiVOIP finishes 
   rebooting the upgrade is complete.



FTP Upgrade:
1. Set a password on the MultiVOIP if one doesn't already exist. This can be done using the 
   Web Browser menus or the MultiVOIP Software via a serial port. Note the default IP Address
   of the MultiVOIP is 192.168.3.143.

2. Unzip the "6_11_41-30_nov_2015.zip" file.

3. Using a ftp client, upload the file "mvpt1ftp.bin" you unzipped in the previous step to
   the IP Address of the MultiVOIP. This should be transferred to the root folder, which 
   normally is the default folder on connection. After uploading the bin file the MultiVOIP
   will reboot. When the boot light turns off, go to the next step.

4. Using a web browser connect to the MultiVOIP and check configuration/system information
   and confirm firmware version as 6.11.41.
