MultiVOIP Firmware v6.11.38

This firmware is for models MVP210/410/810 and is based on the v6.11.22 firmware.

Bug Fixes
- Fixes for Web Interface compatibility issues with Java 7 and later versions.


Note: Depending on the version of Java installed, you may need to change your Java Security level to "Medium" 
to access the MultiVOIP. If you see the message "Application Blocked by Security Settings" then
you will need to set the Java security level to Medium while configuring the MultiVOIP.
To do this go to Control Panel and select Java. The Java Control Panel will come up, select the 
Security tab, move the slider to Medium, and click Apply. It is recommended to set the Java 
Security back to High you are done configuring the MultiVOIP.


Update Instructions
If installing using the MultiVOIP Software on a PC with a serial port follow the 
"MultiVOIP Software Upgrade" instructions, otherwise follow the "FTP Upgrade" instructions.


MultiVOIP Software Upgrade:
1. Install the MultiVOIP v6.11.22 Software, if not already installed. 
   This can be found at the link below.
   ftp://ftp.multitech.com/multivoip/6.11.22-11-Jun-09.zip

2. Connect the MVP210/410/810 to the PC serial port and power it on, if not powered on already.
   Note the USB to serial convertors may not work with MultiVOIP Software.
   When the boot light is off, go to the next step.

3. Run the MultiVOIP Software's "Configuration" before upgrading and take note of the current settings.
   Note the settings should be retained during the upgrade.

4. Unzip the "6_11_38-12_jun_2014.zip" file to a known location.

5. Run the MultiVOIP Software's "Download Firmware" and when prompted to select the "*.BIN" file, 
   browse to the "mvp-06_11_38.bin" file you unzipped in the previous step and click open.

6. The Download Firmware process will take several minutes. When the MultiVOIP finishes rebooting 
   the upgrade is complete.



FTP Upgrade:
1. Set a password on the MultiVOIP if one doesn't already exist. This can be done using the 
   Web Browser menus or the MultiVOIP Software via a serial port. Note the default IP Address of the MUltiVOIP is 192.168.3.143.

***ONLY PERFORM STEP 2 IF CURRENT FIRMWARE IS 6.04 or EARLIER***
2. If version x.04 or earlier, ftp the file "mvpt1ftp.bin" from the link
   ftp://ftp.multitech.com/engineering/unofficial-releases/MultiVOIP/NGAV/javafixes/smooth%20file%20for%20ftp%20upgrade/mvpt1ftp.bin.


3. Unzip the "6_11_38-12_jun_2014.zip" file.

4. Using a ftp client, upload the file "mvpt1ftp.bin" you unzipped in the previous step to the IP Address of the MultiVOIP.
   This should be transferred to the root folder, which normally is the default folder on connection. After uploading the 
   bin file the MultiVOIP will reboot. When the boot light turns off, go to the next step.

5. Using a web browser connect to the MultiVoIP and check configuration/system information and 
   confirm firmware version as 6.11.38.
   Note: If upgrading from an earlier version, the firmware version may display as 6.07.38 or 6.06.38 instead of
   6.11.38 when FTP is performed, this is OK, .38 is the identifier.