*****************************************************
* MTR-X Firmware 3.6.0 Release Notes                *
*****************************************************
Contents:
1) Models Covered By This Firmware.
2) Firmware Upgrade Procedure.
3) Engineering Release Notes for Customer.
4) Support Information.

****************************************************
*    Models Covered By This Firmware               *
****************************************************
- MTR-C2-x
- MTR-EV3-x
- MTR-G3-x
- MTR-H5-x
- MTR-H6-x
- MTR-LAT1-x
- MTR-LEU1-x
- MTR-LVW2-x

****************************************************
*    Firmware Upgrade Procedure                    *
****************************************************
Upgrading to 3.6.0.

WARNING: If firmware upgrade indicates it failed, then DO NOT power cycle, power off or reboot the MTR!
Try the firmware upgrade again. If it fails again, then keep trying or possibly retry with an older
version, but do NOT power cycle, power off or reboot!
Firmware can be found in the following location. Make sure you use the file that is appropriate for your model:
--> ftp://ftp.multitech.com/wireless/mtr/
----"MTR-x" firmware is for the 2G/3G models (C2, EV3, G3, H5, H6).
----"mtr-2g-3g" firmware is for the 2G/3G models (C2, EV3, G3, H5, H6).
----"mtr-lte" firmware is for the LTE models (LAT1, LEU1, LVW2).

NOTE:
Backup your configuration before performing this upgrade. If the login page does not show up
after a firmware upgrade, wait an additional 5 minutes. If the version does not show the latest,
then the upgrade was not successful, try to perform the upgrade again.

NOTE:
To upgrade using the MTR Web UI to MTR 3.6.0 you MUST be running at least MTR 3.4.5 firmware.
To upgrade from a previous firmware, upgrading to MTR 3.4.5 is necessary before upgrading to MTR 3.6.0.

1) Save the firmware binary file to a directory on your workstation.
2) Using the workstation browser, enter the IP address of the MTR (i.e. http://192.168.2.1).
3) Login as admin and enter the admin password.
4) Click "Administration" tab on left side menu bar.
5) Click "Save/Restore".
6) Click "Save Configuration to File" to save a backup file. A popup window will appear.
7) Select "Save File" and click "OK" button.
8) Now click "Firmware Upgrade" tab on left side menu.
9) Click the Browse button and select the latest version of BIN file,
   rcell-mtr-upgrade_3.6.0.bin (non-LTE) or rcell-mtrv1-upgrade_3.6.0.bin (LTE).
10) Click the "Start Upgrade" button. Confirm the 5 minute "OK" button.
11) Wait for the unit to upgrade and reboot automatically.
12) Again, browse to the IP address and verify the Main or Home Page indicates the correct version, 3.6.0.

****************************************************
*    Engineering Release Notes for Customer        *
****************************************************
-----------------------------------------------------
MTR firmware 3.6.0 - March 2017
-----------------------------------------------------
Changes made since release 3.5.6:
- Implment WWAN0 driver support on LTE products.
- Implement SNMP Traps and Noficiations.
- Implement Open VPN Client.
- Add SMS Commands for Serial and WiFi.
- Add Time Stamps to SMS Command responses.
- Implement additional Notifications.
- Various Help Content updates.
- Update Radio Status information.
- Update Wake On SMS settings.
- Update to OpenSSL 1.0.2k.
- Properly configure IPV4V6 for LVW2.
- Added support for both radio-cmd and radio_cmd.

Bug Fixes since release 3.5.6:
- Update LAT1 and LVW2 behavior when SIM requires PIN.
- Remove Diversity checkboxes on LTE products.
- Increase Annex Client cellular traffic statistics max value.
- Update signed Certificate support.
- Fix Debug PING to use br0 instead of eth0.
- PAP/CHAP Authentication updates.
- IE11 Flash Upgrade no longer forces command.json download.

Known Issues in 3.6.0:
- On MTR-EV3, continuous ringing of Wake On Call prevents cellular wake up.
- In Serial Modem mode, using +FTP command for files greater than 2 MB, may
  experience data loss.
- In Serial Modem mode, DCD and DSR LED's may not function properly.
- On MTR-EV3, Us Cellular approval updates required.
- Known SMS Command API issues.
- On MTR-LVW2, certain newer Verizon SIM's do not support SMS.
- On MTR-LVW2, received SMS's greater than 140 characters may be limited to 140.

****************************************************
*      Support Information                         *
****************************************************
Multi-Tech provides free technical support for your product. To obtain this support,
we suggest you create a support case on our Support Portal at:
https://support.multitech.com

If internet is not available, try one of our numbers:
U.S. & Canada number: 763-717-5863
Answered Monday - Friday
8:00 am to 5:00 pm Central Time (Daylight savings observed when in effect)

International number: +763-717-5863
Answered Monday - Friday
8:00 am to 5:00 pm Central Time (Daylight savings observed when in effect)

EMEA    support@multitech.co.uk         +(44) 118 959 7774
U.S.    support@multitech.com           800-972-2439 or
(and Rest of World)                     +763-717-5863

Replacement Parts and Accessories
For replacement parts and accessories, contact Multi-Tech at:
(888) 288-5470, option 3 or +1 (763) 785-3500

US Mail Address:
  Multi-Tech Systems, Inc.
  2205 Woodale Drive
  Mounds View, MN 55112
  USA

::Form Version R2014-03-27::