*****************************************************
* MTR-x Firmware/Software Release Notes             *
*****************************************************

Contents:
1) Models Covered By This Firmware/Software
2) Firmware/Software Upgrade Procedure
3) Engineering Release Notes for Customer 
5) Support Information

****************************************************
*    Models Covered By This Firmware/Software      *
****************************************************
- MTR-C2-x
- MTR-EV3-x
- MTR-G3-x
- MTR-H5-x
- MTR-H6-x
- MTR-LVW2-x
- MTR-LAT1-x
- MTR-LEU1-x

****************************************************
*    Firmware/Software Upgrade Procedure           *
****************************************************
Upgrading to 3.4.2

Note: Backup your configuration before performing this upgrade.  If the firmware upgrade fails, 
or it does not show the login page again, wait an additional 5 minutes. Power off and on the MTR 
and web to the MTR to check the version. If the version does not show the latest, then the  
upgrade was not successful. Try to perform the firmware upgrade again by repeating all the steps.

1) Save the firmware binary file to a directory on your workstation
2) Using the workstation browser, enter the IP address of the MTR (i.e. http://192.168.2.1).
3) Login as admin and enter the admin password.
4) Click "Administration" tab on left side menu bar
5) Click "Save/Restore"
6) Click "Save Configuration to File" to save a backup file. A popup window will appear
7) Select "Save File" and click "OK" button
8) Now click "Firmware Upgrade" tab on left side menu
9) Click the Browse button and select the latest version of BIN file, rcell-mtr-upgrade_3.4.2.bin or rcell-mtrv1-upgrade_3.4.2.bin
10) Click the "Start Upgrade" button.
11) Wait for the unit to upgrade and reboot automatically.
12) Again, browse to the IP address and verify the Main or Home page indicates the correct version, 3.4.2.


****************************************************
*    Engineering Release Notes for Customer        *
****************************************************

------------------------------------------------------------
MTR SW 3.4.2 - April 15th, 2016
------------------------------------------------------------

Changes made since release 3.3.2:

Bug Fixes:
* For LVW2, special characters like @ $ not sending through sms properly
* Fix restart via WAN redirects to LAN
* Do not allow SMS and wake-on-sms to be enabled at the same time on CDMA radios
* MTR-C2 MEID may display as hex or decimal (now always hex)
* Notify user when downloading a configuration with pending changes
* Fix wakeup on call hover help
* Fix: Able to create two tunnels with the same end points and LAN networks
* Fix: Tunnel must not be allowed configuration if Remote LAN is equal to Local
* Fix: Deleting Cellular History illuminates Save and Restart button
* Fix: Serial Port as client will not reset a broken TCP connection when ALWAYS ON is set for Connect/Disconnect Method
* Fix: Missing Button Status & Logs | Statistics GRE Tab
* Fix: Serial Port UDP client - DTR Assert not working in some situations
* Fix: Serial-IP Config - UI issue with connection termination

Features/Enhancements:
* Notifications (email and SMS) for Data Usage, Reboot, Signal Strength
* Upload System Logs to DeviceHQ
* SMS Commands (reboot & check-in to DeviceHQ)
* Serial Modem Mode
* Added SMS support for all CDMA radio models including C2, EV3 and LVW2
* Remove Firewall restriction where multiple rules have same destination port and interface
* Removed menu link for Initial Setup Wizard.  A factory default is now required to change between modes (Router, PPP IP Passthrough, Serial Modem Mode)
* Updated built in help content

Known Issues:
* Serial Modem Mode:
    * In Serial Modem Mode, there is a known issue with data loss when using the AT+FTP command.
    * In Serial Modem Mode, the DCD and DSR do not work properly.  The CD LED may not reflect the DCD correctly.
* Wake-On-SMS: On the LVW2 model, wake-on-sms may not work the first time after boot.

Additional changes made since release 3.2.3:

Bug Fixes:
* Added ability to set "infinite" DHCP lease time in web UI
* Fixed UI quirk around Serial-IP configuration
* Added ability to manually configure DNS servers in Passthrough mode
* RX monitor fixed in Passthrough mode
* Fixed WAN failover logic
* Fixed prompt to disable bluetoothIP when enabling serialIP
* Fixed notification messages when saving Remote Management settings\
* Fixed PPP connection for G3 radios 

Features/Enhancements:
* Added limited IPv6 support (IP Passthrough mode only)
* Added "on demand" option to the Serial IP and Bluetooth IP features
* Added option for web gui to use http by disabling the http to https redirect
* Added info popup when enabling wake-on-call about probably wanting Dial-on-Demand

****************************************************
*      Support Information                         *
****************************************************
Multi-Tech provides free technical support for your product as well as paid phone support.

Free technical support via Multi-Tech Online Support Portal at:

https://support.multitech.com
To obtain this support, use one of the following contact options:

U.S. & Canada number: 763-717-5863
Answered Monday - Friday

Phone calls are handled in the order they are received. Free support is not offered by phone, but staff will help create a case and/or set up paid phone support.

8:00 am to 5:00 pm Central Time
(Daylight savings observed when in effect)

International number: +763-717-5863
Answered Monday - Friday
8:00 am to 5:00 pm Central Time
(Daylight savings observed when in effect)


EMEA    support@multitech.co.uk         +(44) 118 959 7774
U.S.    support@multitech.com           800-972-2439 or
(and Rest of World)                     +763-717-5863


Replacement Parts and Accessories

For replacement parts and accessories, contact Multi-Tech at:

(888) 288-5470, option 3
       or
+1 (763) 785-3500

US Mail Address:

Multi-Tech Systems, Inc.
2205 Woodale Drive
Mounds View, MN 55112
USA

::Form Version R2011-12-08::


