Firmware Version : 4.09.0C
Firmware Date : 10-NOV-2006

Frimware Description :
DV firmware with Audit support for ISDN.

Procedure to get Audit:
When call fails, do the following:
1) Use HyperTerminal to capture to a file.
2) Type '!' (without the quotes)
3) Type 'a' (without the quotes)
4) Press any key when ready to capture the output from the VoIP (it will dump out a lot of data)
5) When the VoIP is finished dumping data it will give you another prompt. Type 'x' to exit.
6) Stop the capture to the save file.
7) Decode capture file with decode batch file found with Xview utility.(Xview attached)
7) It may be best to reset the VoIP since dumping the audit information prevents the VoIP from responding to the ISDN network.

changes made on top of 4.09.0B 

release history checked into SVN

Regards,
Umesh