Firmware Version : 4.09.0R
Firmware Date : 05-JAN-2007

Frimware Description :

Firmware for customer Dmitry Petrov: Changes for NAME and TEL fields filling from Display IE and Calling party name IE as per his requirements. 

logic:

TEL field:

1)if source number sent from PRI(calling part number), then use source number , else
2)Use proxy enabled and proxy call, then use Sip proxy Username, else
3)Use remove prefix for that channel, else
4)Use GWname, else
5)Use Unknown.

Name field:
1)if source name(Display IE) sent from PRI, then use that name to fill , else
2)IF proxy enabled and Proxy call, use SIP proxy Username(string, be it name or number), else
3.1)Fill Gateway name, else
3.2)Use inbound description field, else
3.3)Use detected source phone number(calling part number), else
3.4)Use remove prefix, else
3.5)Use Unknown.


changes done on top of 4.09.0Q.

release history checked into SVN

Regards,
Umesh