
How to perform FW update

download, setup and run Web server software to host the patch file
https://www.rejetto.com/hfs/
check make sure it is listen on the Sequans ethernet virtual ethernet 192.168.16.x

put the patch file into the web server folder
CB610L-49444.sfp

bring up terminal and issue AT Command to apply the patch.  IP and port should match up with web server above
AT+SQNSUPGRADE="http://192.168.16.199/CB610L-49444.sfp",1,15


new FW version ATI
ati
SEQUANS Communications
CB610L
UE4.2.2.0-49444

