*************************************************************************
*                                                                      	*
*  DiskOnChip(R) TrueFFS(R) Uilities package             		*
*                                                                      	*
*  Version 6.3.2.12 Release from  November 30th, 2005			*
*  Based on TrueFFS Version 6.3.2 from  November 30th 2005  		*
*                                                                      	*
*  Copyright M-Systems (c) 2005						*
*                                                                      	*
*  Readme							        *
*                                                                      	*
*************************************************************************

This Package includes the TrueFFS Version 6.3.2 Utilities Package

Package Contents
----------------

Please refer to the attached document: 
DiskOnChip Software Utilities for TrueFFS 6.x - User Manual


Devices Supported by this Version
----------------------------------
	- DiskOnChip G3/P3 family
	- DiskOnChip G3/P3 LP family
	- DiskOnChip H1 family
		- DiskOnChip H1 256MB
		- DiskOnChip H1 512MB
		- DiskOnChip H1T 1GB
	- DiskOnChip G4 family
		
Notes:
	- TrueFFS 6.X supports only SAFTL based devices. Devices supported
	  by TrueFFS 5.x are not supported by this release.
	- DiskOnChip must be formatted when upgrading from TrueFFS 6.3.0 
	  Alpha to 6.3.0 beta and above.
	- DiskOnChip must be formatted when upgrading from TrueFFS versions
	  prior to TrueFFS 6.3.0 beta.
 
Known limitations
-----------------

1. DIMAGE 
	- /verify flag does not verifies IPL and OTP areas.
	- /verifyimg will fail if device was programmed using other platform, than
		verifyimg run.
	- Leave binary partition formatting flag is not supported for binary
	  partition that spans over more then 1 floor.
	- /verifyimg flag does not support rammtd.
	- Get image operation creates an empty file though it fails, when key isn't insterted in protected 
	  partition configuration.
	- Programming target DiskOnChip with locked OTP area using master image file with no OTP 
	  will succeed.

2. DFORMAT
	- Signature, specified for non specified binary partition in the format command is ignored by DFORMAT
	  without any error message. 
	- Read IPL from unformatted DiskOnChip leads to empty file creation. 
	- Using /READ with no /bdkn flag when binary partition with different signature than BIPO, 
	  cause wrong error message ("No Space In Volume").
	- Writing PAged RAM IPL to DiskOnChip G4 prints wrong printout of the IPL size that was actual written.
	- DiskOnChip G4 OTP is not supported.


3. DINFO 
	- Secondary partition information not includes FS number.
	- Shows error message, despite of right logical partitions information. 
	- The size of bdkspl partition shown is the actual capacity of that bdk, and not the size on disk.
	

4. RAM FILE MTD
	- OTW is not supported.
	- DiskOnChip G4 max IPL size in virtual mode is equal to 248KB instead of actual support of 8KB.
	- With Dimage Does not support single floor programming.
	- When IPL is not written or erased, DIMAGE will produce diffrent image file 
	  from real device and RAM FILE produced from RAM FILE MTD device.  Therefore RAM file must 
	  be first unformatted in RAM FILE OF G3 and H1 . 
	  In RAM FILE Of DiskOnChip G4 Dimage will produce differenet images even if RAM FILE is unformatted.

	
	  
	



Contact information
--------------------

Please visit our website for the latest updated information.

	Internet:   http://www.m-systems.com
  	E-mail:	 	info@m-systems.com
  
  	USA:        M-Systems, Inc.
		555 North Mathilda Avenue, Suite 220
		Sunnyvale, CA 94085
		Phone: +1-408-470-4440
		Fax: +1-408-470-4470

  
	Taiwan:     M-Systems Asia Ltd.
		14 F, No. 6, Sec. 3
		Minquan East Road
		Taipei, Taiwan, 104
		Tel: +886-2-2515-2522
		Fax: +886-2-2515-2295


	Japan:      M-Systems Japan Inc. 
                Asahi Seimei Gotanda Bldg., 3F
                5-25-16 Higashi-Gotanda
                Shinagawa-ku Tokyo, 141-0022
                Phone: +81-3-5423-8101
                Fax:   +81-3-5423-8102
  
	China:      M-Systems China Ltd.
		Room 121-122
		Bldg. 2, International Commerce & Exhibition Ctr.
		Hong Hua Rd. 
		Futian Free Trade Zone 
		Shenzhen, China
		Phone: +86-755-8348-5218
		Fax: +86-755-8348-5418


	Europe:	    M-Systems Ltd. 
                7 Atir Yeda St. 
                Kfar Saba 44425, Israel
  		Tel: 972-9-764-5000
  		Fax: 972-3-548-8666
  
  	© 2005 M-Systems Flash Disk Pioneers, Ltd. All rights reserved.
  	This document is for information use only and is subject to 
  	change without prior notice. M-Systems Flash Disk Pioneers Ltd. 
  	assumes no responsibility for any errors that may appear in this
  	document. No part of this document may be reproduced, transmitted,
  	transcribed, stored in a retrievable manner or translated into
  	any language or computer language, in any form or by any means, 
  	electronic, mechanical, magnetic, optical, chemical, manual or 
  	otherwise, without prior written consent of M-Systems.

  	M-Systems products are not warranted to operate without failure. 
  	Accordingly, in any use of the Product in life support systems or
  	other applications where failure could cause injury or loss of
  	life, the Product should only be incorporated in systems designed
  	with appropriate and sufficient redundancy or backup features.
  	Contact your local M-Systems sales office or distributor, or visit
  	our website at www.m-sys.com to obtain the latest specifications 
  	before placing your order.

  	M-Systems® is a registered trademark. DiskOnChip®, DiskOnChip
  	Millennium®, DiskOnKey® and TrueFFS® are registered trademarks
  	of M-Systems. DiskOnKey MyKey™, FFD™, Mobile DiskOnChip™ and
  	SuperMAP™ are trademarks of M-Systems. Other product names mentioned
  	in this document may be trademarks or registered trademarks of their
  	respective owners and are hereby acknowledged.
