*************************************************************************
*                                                                      	*
*  DiskOnChip(R) TrueFFS(R) Uilities package             		*
*                                                                      	*
*  Version 6.3.2.12 Release from  November 30th, 2005			*
*  Based on TrueFFS Version 6.3.2 from  November 30th 2005  		*
*                                                                      	*
*  Copyright M-Systems (c) 2005						*
*                                                                      	*
*  Versions							        *
*                                                                      	*
*************************************************************************

This Package includes the TrueFFS Version 6.3.2 Utilities Package
*************************************************************************

Package Contents
----------------
Please refer to the attached document: 
DiskOnChip Software Utilities for TrueFFS 6.3 - User Manual

version 6.3.2.12 Release
-----------------------
1. Supports the following DiskOnChip Products:
	- DiskOnChip G3/P3 family
	- DiskOnChip G3/P3 LP family
	- DiskOnChip H1 family
		- DiskOnChip H1 256MB
		- DiskOnChip H1 512MB
		- DiskOnChip H1T 1GB
	- DiskOnChip G4 family

2. This Package includes the TrueFFS Utilities Package for DiskOnChip. 
	- DOCSHELL   version 6.3.2.12
	- DFORMAT    version 6.3.2.10
	- DFS        version 6.3.2.10
	- DINFO      version 6.3.2.10
	- DIMAGE     version 6.3.2.11
	- SPLITIMGAE version 6.3.2.9

3. Bug fixes
	All Utilities - Compilation error when disabeling flag HW_PROTECTION .
	Dformat - Format with leave flag did not assign signatures of subpartitions correctly. 
	Dformat - Writing IPL bigger than 14k on DiskOnChip G4 with protection at the same command line failed.
	Dimage  - Using DFS create different images from real device when working with RAM MTD.
	Dimage  - Single floor programing to other floors than the first one failed.
	Dimage  - Image taken from the 2nd floor to fourth floor of DiskOnChip G4 includes the IPL 
		  taken from the first floor.
	Dinfo	- flag /logd didn't show all logical partitions 
	Dinfo	- Secondary logical partition that follows right after extended one cannot be shown 
	  	  by using /LOGD[bdtl][:drive]
	DFS 	- failed when key was inserted though there was no protection.


changes from version 6.3.2.11 beta
--------------------------------------
No changes


changes from version 6.3.2.10 alfa
--------------------------------------
	All utilities - Addition support for DiskOnChip G4 RAMMTD.
	SPLITIMAGE    - Addition support for DiskOnChip G4 cascaded configuration.



changes from 6.3.1.8 - August 31th, 2005
--------------------------------------
	DIMAGE - Maximum bit flips number for EP partition calculation refined
	DIMAGE - Fix bug in verify image functionality
	SPLITIMAGE - progress bar not shown while splitting
	RAM FILE MTD - Registration fixed
	All utilities - Fix functionality of /clfile 
	All utilities - Refined casting for default memcmp() implementation return value.


changes from 6.3.0.3 - July 27th, 2005
--------------------------------------
	ALL utilities - up to 9 command line parameters from each type may be specified 
		fiexd to up to 99
	DFORMAT fail to insert keys to non-first disk partition
	DFORMAT shows wrong IPL length for G3/P3 devices
	DINFO not shows SPL information for H1 devices
	DINFO wrong or no information shown about logical partitions
	DINFO failed to show information about read-protected parititons
	DIMAGE write error not detected on P3 devices due to wrong number of shared sectors
	DIMAGE deletes more units, than required on cascaded device, when partition over floor
	DFS command line parsing bugs
	






For futher utilities description please, refer to the Utilities User Manual


For comments, questions and bug reports, please contact your M-Systems 
representative or e-mail us at techsupport@m-sys.com.

An M-Systems full contact list can be found on our website (www.m-sys.com).




