Overview:

    *
      A very basic Perl code sample that will show how to send a fax to the Multitech Fax Finder device using Web Service API.

Prerequisites:

    * Download and Install Perl Active 5.10.0 at http://www.activestate.com/activeperl
    * Download the Perl sample source code SendFax-Perl.zip here

Notes: The SendFax-Perl.zip contained two files:

    * sendfax.pl
    * schedule.xml

Modify schedule.xml:

Load the schedule.xml file into your favorite editor, find the section below, and modify the fax number to point to your recipient fax number:

<recipient>
...
<fax_number>5138</fax_number>
</recipient>

Save it.

Modify sendfax.pl:

Load up the sendfax.pl file into your favorite editor. Change the following.

Change the path to point to your Perl path.

#!/perl/bin/perl -wT

Change the user name and password.

$request->authorization_basic("admin","admin");

Change the IP address of the following line to point to your Fax Finder’s IP address.

my $request = HTTP::Request->new(POST => 'http://216.133.69.247/ffws/v1/ofax');

Save it. Go to command prompt and cd to the folder where it contained the sendfax.pl file and type:

perl -T sendfax.pl

Now, if you web into your FaxFinder device and go to Status & Log -> Fax Status, you should be able to see the Fax Finder is sending out a fax.